ITEM 625 NO. 4 AWG 600 VOLT DISTRIBUTION CABLE, AS PER PLAN

INSULATED CABLE SHALL BE USED FOR THE GROUND WIRE (GND) WHERE INDICATED FOR SYSTEM GROUNDING AND BONDING. THE JACKET OF THE GND WIRE SHALL BE GREEN WITH TWO YELLOW STRIPES/TRACERS. THIS GND WIRE SHALL BE SEPARATE FROM THE GROUND ROD WIRE, BUT SHALL BE CONNECTED TO THE SAME GROUNDING BOLT USED FOR THE GROUND ROD WIRE ATTACHMENT AT THE POLE. THE GND WIRE SHALL BE TAGGED AS "GND SYS" AT ALL POLE LOCATIONS, PULL BOXES, AND & CONTROL CABINETS. *10/6/15*