## ITEM 625 PULL BOX, MISC.: PULL BOX ADJUSTED TO GRADE

*Instructions to designer: This item is only applicable to 725.08 concrete pull boxes (Type 4021, 4022, or 4023). Existing concrete square pull boxes with metal frames and lids and 725.06 polyconcrete pull boxes shall not be adjusted to grade and shall instead be replaced.*

UNDER THIS ITEM OF WORK, the existing pull box shall be ADJUSTED SO THAT THE PULL BOX LID IS AT PROPOSED GRADE. ADJUSTMENT SHALL BE PER 604.03.b.

Verify that the EXISTING pull box lid frame structure is free of cracks or other defects, securely fastened to the pull box, and that a seal is present between the two materials.

Verify that the pull box lid is in good condition and is properly seated within lid frame upon closing of pull box lid.

if the engineer determines the pull box lid frame structure or lid are in poor condition, these items shall be replaced prior to adjusting the pull box to grade.

PAYMENT SHALL BE PER ITEM 625 AND SHALL BE MADE AT THE UNIT PRICE BID PER EACH PULL BOX ADJUSTED TO GRADE AND SHALL INCLUDE FURNISHING ALL MATERIALS, EQUIPMENT, LABOR AND INCIDENTALS NECESSARY TO COMPLETE THE WORK AS SPECIFIED. 7/1/24