## ITEM 632 CONDUIT RISER, 2", 725.04, MODIFIED, AS PER PLAN

IN ADDITION TO THE REQUIREMENTS OF 632 AND 725, THE CONDUIT RISER FOR FIBER OPTIC CABLES SHALL BE AS DETAILED ON STANDARD DRAWING 4602. 6/22/21