**ITEM 632 PEDESTRIAN SIGNAL HEAD, AS PER PLAN**

*Designer instructions: this note is to be used for Easton or Polaris projects only. There is no as per plan note for standard black pedestrian signal heads.*

In lieu of the paint color requirements of 732.05, the housing and two-hinged type brackets shall be gloss blue per Federal Standard #595B, color #15048. 3/4/20