**TRAFFIC CONDUIT DAMAGE**

THE EXISTING TRAFFIC CONDUIT BANK AND CONDUITS SHALL NOT BE DISTURBED. CAUTION SHALL BE USED TO AVOID DAMAGING EXISTING TRAFFIC CONDUIT BANK, CONDUITS, AND CABLES CONTAINED WITHIN. IF NECESSARY, THE CONTRACTOR SHALL PROPERLY SUPPORT THE TRAFFIC CONDUIT BANK AND CONDUITS DURING CONSTRUCTION. TRAFFIC CABLES SHALL NOT BE DISCONNECTED OR TAKEN OUT OF SERVICE.

THE CONTRACTOR SHALL BE RESPONSIBLE FOR THE REPLACEMENT OF ANY DAMAGED CONDUIT BANK OR CONDUITS, AS DETERMINED BY THE CITY OF COLUMBUS DIVISION OF DESIGN AND CONSTRUCTION. ANY CONCRETE ENCASEMENT DAMAGED OR REMOVED FROM THE CONDUIT BANK SHALL BE REPLACED. CONCRETE ENCASEMENT SHALL BE SEPARATE FROM ANY BACKFILL MATERIAL OR ADJACENT ENCASEMENT MATERIAL.

THE CONTRACTOR SHALL BE RESPONSIBLE FOR THE REPLACEMENT OF ANY DAMAGED CABLE, AS DETERMINED BY THE CITY OF COLUMBUS DIVISION OF DESIGN AND CONSTRUCTION. NO SPLICES IN TRAFFIC CABLE ARE PERMITTED, SO THE ENTIRE RUN OF CABLE FROM DEVICE TO DEVICE MUST BE REPLACED IF CABLE DAMAGE OCCURS. 4/28/16