**Item 1620 Misc.: Termination Panel, 24 Fiber, with 250 ft Drop Cable**

**Item 1620 Misc.: Termination Panel, 24 Fiber, with 500 ft Drop Cable**

The termination panel shall be furnished and installed in the traffic signal controller cabinet at the location shown on the plans. The termination panel ASSEMBLY SHALL BE BY CORNING INC AND INCLUDE A WALL-MOUNTABLE SINGLE-PANEL HOUSING (SPH) AND a pre-connectorized drop cable OF THE SPECIFIED LENGTH.

The work as described will be measured as one unit for each installation specified, and shall include all materials, LABOR, equipment, testing, and incidentals, complete in place. Terminations, connections, and other miscellaneous items and materials shall be incidental to this work and no separate payment will be made. 3/28/25