**ITEM 625 MISC.: LUMINAIRE, LED, 120 V, TEARDROP (BLACK)**

LUMINAIRES INSTALLED ON COMBINATION TRAFFIC SIGNAL SUPPORTS SHALL BE PER CITY OF COLUMBUS MIS-801 EXCEPT THE VOLTAGE SOURCE SHALL BE 120 VAC. THE LUMINAIRE HOUSING SHALL BE COATED TO MATCH ITS RESPECTIVE COMBINATION SIGNAL SUPPORT.

PAYMENT SHALL BE AS PER ITEM 625. *7/1/24*