**ITEM 632 LOOP DETECTOR UNIT, AS PER PLAN**

THE LOOP DETECTOR UNIT SHALL BE A SOLID STATE, 2 CHANNEL, SHELF MOUNTED INTERSECTION DEVELOPMENT CORPORATION (IDC) MODEL 921-2TCSS-1 OR RENO A&E MODEL T210-SS.

PAYMENT FOR THIS ITEM IS FOR EACH LOOP DETECTOR UNIT INSTALLED IN THE TRAFFIC SIGNAL CONTROL CABINET.*1/30/19*