**ITEM 632 LOOP DETECTOR UNIT, AS PER PLAN**

THE LOOP DETECTOR UNIT SHALL BE A SOLID STATE, 2 CHANNEL, SHELF MOUNTED INTERSECTION DEVELOPMENT CORPORATION (IDC) MODEL 921-2TCSS-1, RENO A&E MODEL T210-SS, OR EBERLE DESIGN INC. (EDI) MODEL ORACLE S2ECS.

PAYMENT FOR THIS ITEM IS FOR EACH LOOP DETECTOR UNIT INSTALLED IN THE TRAFFIC SIGNAL CONTROL CABINET.  *1/30/19*