**ITEM 632 STRAIN POLE FOUNDATION (BY DEPTH), AS PER PLAN**

**ITEM 632 SIGNAL SUPPORT FOUNDATION (BY DEPTH), AS PER PLAN**

*Instructions to designer: This note and pay item is only used when a deep foundation is required and approved by the City signal reviewer due to a utility located within 5 ft of a proposed signal pole. See SCD 4160 note 14.*

FOR SIGNAL POLES MOUNTED TO DEEP FOUNDATIONS CONSTRUCTED UNDER THIS ITEM, THE aluminum pole identification tag, as required AND IN ACCORDANCE WITH 732.11 and 732.12, shall also be labeled with “deep foundation” followed by the depth of the foundation (e.g. deep foundation, 18 ft). THE FOUNDATION SHALL BE CONSTRUCTED IN ACCORDANCE WITH 632.14, SCD 4160, AND SCD 4161. 5/15/18